**Project plan: Mechanical keyboard**

Pyry Koivistoinen, 100648540

Abbreviations

MCU, TKL PCB, CAM, QMK

Abstract

This project is about designing and manufacturing a mechanical keyboard from scratch. Project includes mechanical and electrical design with some programming. The aim of the project is to make a functional keyboard, learn mechanical design in the limits of what is possible to manufacture, learn electrical design and about keyboard matrices.

Introduction

* Motivation, why did I decide to make this project
  + I had over 7 years old Rantopad MXX keyboard and I grew tired of the loud switches it had. I mostly use a keyboard for typing, so the switches need to feel good, and they need to be silent. I had been planning on buying a new mechanical keyboard soon, but I decided it would be more fun to try to build one myself instead of buying. I could learn mechanical and electrical design at the same time and create something myself from the scratch.
* Inspiration
  + Early inspiration for this project was Varmilo VA88M. Its sleek and simple design pleased the eye, and it does fit well with simplified pc aesthetics. Keyboard layout is TKL, tenkeyless, or 80%, meaning that it doesn’t have number pad on the right side of the keyboard. Example of this board can be seen in **figure.** The color theme in CMYK model was pleasant: White background and colorful accents. Another inspiration came from TGR Jane v2. The case’s shape and angle looked good. Additionally, Jane v2 had a F13 extra function key, that seemed like a nice addition. Jane v2 uses ANSI layout for the keys which looks more compact than ISO layout.
* Requirements and budget
  + When doing the research, Varmilo VA88M was around 120 euros. The plan was to aim at similar price, keeping in mind that there might be mistakes in the design process, and redesigns would cost more.
  + More expensive keyboard use aluminum or brass cases or have extra weights attached. This keeps the keyboard steady while typing, makes the case more rigid, which reduced differences in key presses and makes the overall quality feel better.
  + **Tästä puuttu jotain välistä, miten transition requirementteihin?**
  + Most important requirements for the keyboard are as follows:
    - Heavy aluminum case.
    - TKL with ANSI layout.
    - Sleek and aesthetically good-looking design.
    - Tactile and silent switches.
    - USB C cable.

All requirements should be met. Keyboard assembly should be as cheap as possible when requirements are met.

* Tools in use?
  + For this project it was necessary to have a way to machine the case and assemble the PCB. For my disposal there was a machining center and soldering equipment.

Methods, mechanical section

* Component design
  + Component design was done by using Siemens NX and PCB design using KiCad.
  + Case
    - I wanted to make the case from one piece to ease the manufacturing. The weight of the keyboard was important. It needed to feel heavy, so the keyboard stays firmly in place and doesn’t move around while typing. The whole construction needed to feel sturdy. Material chosen for the case was Al6082 for its accessibility and mechanical properties. The estimated weight for the case would be **\_\_\_ g.** Keyboard layout is TKL, tenkeyless, or 80%. This layout was chosen because of its compact size, nice aesthetics and there was no need for number pad in daily use.
    - Securing: Case acts as a base for the whole keyboard, so all other components needed to be able to be secured to the case. For securing method, four shafts that had a thread inside were machined inside the case. Keyboard’s PCB and plate were constrained with the holes and pressed down with bolts that prevented the components from moving. Cross section of the constraining method can be seen in **figure.**
    - Typing: For best typing experience the keys need to be angled slightly towards the typer, usually angle being 5-7 degrees. Since the case was made in one piece, everything inside it had to be angled. Limiting factor was the available aluminum billet, that had a height of 30 mm. Inside these limits the case angle was chosen to be **5,7 degrees.**
  + Switches
    - My previous keyboard had Kailh Blue switches. The switch type is tactile and loud. I like the tactical bump while typing but prefer more silent keys.
    - The best option was Holy Panda switches which are advertised as the most tactile switches in the world [1]. There was no opportunity to test the switches out, but based on the sound tests they seemed good. Unfortunately, whole set would’ve costed 70 euros, which made them inaccessible for this project.
    - Next option was Cherry MX Brown switches. They are tactile, more silent compared to blue switches and very common. Because of their commonness they are accessible with competitive price.
    - One of the requirements for the keyboard was to make it as cheap as possible. Because of this it was decided to buy old keyboard which had the desired switches instead of buying the switches new. Cheap used keyboard was found from tori.fi that had the desired switches. It was bought and switches removed. The PCB also had leds for every key, which can be used as indicator leds.
  + Plate
    - Plate is the piece locking the keycaps in place and keeping them from moving. Plate is the most top part and acts as a lid for the keyboard and will be visible in some parts. Since the case is made from aluminum, the plate should be too. This matches the materials and gives better structural properties compared to e.g. PLA plastic.
    - Plate had to be 1,5 mm thick, so the switches can lock properly. Holes were done according to Cherry’s datasheet [2].
  + Keyboard units
    - One key is 1 unit etc. :D
  + Switch stabilizers
    - For longer keycaps that are more than 2 units, it is required to have switch stabilizer. The stabilizer consists of two buttons and a rod connecting them. When the key is pressed, the keycap is supported from the whole area, and it makes the keypress more stable and haptically better.
    - Switch stabilizers were snapped in place to the plate to make them rattle less.
  + Keycaps
    - Varmilo VA88M had a pleasant color combination, so it was chosen to have something similar. The bright colors were too intensive, so it was chosen to have a white base with blue or green pastel accents. In ebay there was a PBT keycap set that had the correct color theme. The selected keycap set can be seen in **figure X.**

Methods, electrical section

* Requirements
  + It is possible to buy readymade keyboard PCBs, but I wanted to make my own, because:
    - I have some experience in PCB design.
    - It is cheaper to make one yourself.
    - I wanted to know how keyboards work.
    - I designed the case, so I needed the PCB to fit and be able to be secured to the case.
* Design
  + I didn’t know where to start with the PCB design, so I searched online for open-source keyboard projects. I found one that was based on Hineyboard h88. Differing from normal TKL, this keyboard had F13 extra function key.
* Keyboard matrix
  + Why matrix: There is 87 keys in TKL keyboard and to have a functional keyboard, every key press should be detected. In this case the keyboard would require a microcontroller that has 87 input pins. Such microcontrollers exist, but there is much more efficient way of detecting key presses, which comes in a form of matrix.
  + How matrix works:
  + What diodes does in a matrix
  + Explain how this keyboards matrix is set up
  + It would be inefficient to use separate diode of every individual switch. This is why BAV70 diodes were chosen. They include two diodes in compact SOT-23 package, which reduces the number of components on the board, making routing traces easier.
* Microcontroller
  + What it is: The microcontroller or MCU was Atmel Atmega32u4. Package was.
  + Why it was chosen: The MCU is extensively used in keyboard projects. The number of IO pins was enough for rows and columns. Because it is common, it is widely available and cheap to purchase.
* Component manufacturing
  + Case and jig CAM
    - All mechanical parts were designed using Siemens NX. CAM was done using Siemens CAM feature. Case had an angle in the bottom which meant that the piece had to be turned during machining. The top and the sides needed to be machined in one go.
    - To do that, a jig piece needed to be designed. The jig piece was designed to hold the case from the screw holes and line it perpendicular with the machine z-axis. The mill turned b-axis 5,7 degrees and the case bottom and sides was machined. **Figure x** shows the jig with the case attached.
  + Case machining
    - Case was machined using HAAS UMC750 milling center. The machine has a capability of milling in five degrees of freedom, but only 3 was needed. Forth dof was helpful for cutting the angles. The milling process can be seen in **figure x.** Since the case was to be machined from one piece, thebillet size had to be greater than the case. A billet with size of **xxx** was used.
  + Plate laser cutting
    - The plate design was verified with a 3d-printed model. It had to be in two parts because of 3d-printer space limitations. Test plate fit with some filing, and switches aligned well with the PCB. Next the plate was cut out of aluminum with laser cutting. Laser cutter used was **hhh.**

Programming section

* Flashing MCU
  + Arduino ISP
    - The microcontroller didn’t have a bootloader preinstalled. Bootloader is a program that allows the loading of other programs to the microcontroller via more convenient interface like USB cable. This is why the keyboard was designed with ISP communication protocol pins on the board, making it more convenient to connect the keyboard to an Arduino UNO and flash it with a bootloader. After the microcontroller had the bootloader installed, it was ready to be flashed with the keyboard code.
  + QMK MSYS
    - First the keyboard code had to be compiled using QMK firmware. Because of the changes in matrix layout, the matrix needed to be configured again. This happened by modifying the keyboard config.h and h88.h files. In config.h file the right rows and columns were defined for right pins in microcontroller. In h88.h file the correct keyboard layout was modified to match with the keyboard’s rows and columns. After modifications were done, the code was compiled as .hex file.
* QMK Toolbox
  + QMK toolbox was used to flash the microcontroller. Before the microcontroller had any code written on it, it was already in programming mode. After the first flash the programming mode was toggled by grounding the reset pin twice in a row. This was made easy by implementing a reset switch on the keyboard PCB. QMK Toolbox detected the microcontroller, and the code was flashed to the keyboard. After this the keyboard appeared in windows devices as a device h88. Key presses were tested using tweezers by connecting rows and columns together one by one. The program for monitoring the key presses was Switch Hitter.
* Mapping keys
  + In QMK configurator the keys can be configured to whatever desired. In this project there was no need to configure anything else than the extra function key F13. This key was assigned as a sleep button: When pressing the sleep button, it will put the computer to sleep mode.

Discussion

* How did the project go?
  + Two versions were done of the keyboard PCB.
* What was the price?
  + The budget was set around the price of Varmilo VA88M, which was 120 euros at the time of the project. The total price for one assembly of the keyboard can be seen in **table x.**

|  |  |
| --- | --- |
| **Component** | **Price paid (€)** |
| Case | 0,00 € |
| Plate | 0,00 € |
| Switches | 23,00 € |
| Keycaps | 21,20 € |
| PCB | 20,42 € |
| Components | 16,61 € |
| USB-C cable | 6,30 € |
| Total: | 87,53 € |

* + Case and plate didn’t cost anything since it was possible to utilize available aluminum and machinery for free. The price quotation from Hubs.com for the case machined would’ve been 254 € which was completely out of budget. In addition, plate would’ve costed 20,85 €Xometry.com, bringing the total price to362,38 €**.** One possible way to stay under budget if machining is not an option would be to 3d-print the case and add dense material as weight to simulate the wanted properties.
  + The keyboard PCB needed to be ordered twice because of the matrix mistake in version one. This added 20 euros to the total price, which wasn’t considered in the total price.
  + Price for one assembly of the keyboard stayed inside the budget limit, but ordering everything was not a viable option.
* How does it look and function?
  + The final product was functional keyboard which can be seen in **figure x.** Few problems still exist which are explained below but can be fixed in version two.
  + Pictures and video?
* What could be improved?
  + Teams list
  + Securing to case with slimmer and more stable screw heads
  + Better typing angle with same case outside design? Onko mahdollista tai kannattavaa?
* Problems faced:
  + Ver1 matrix fukked
    - The keyboard layout was what I wanted, the board looked good, and the project well made, so I decided to order the board from JLCPCB. While testing the board, it turned out that the switch matrix was completely off, every second key was the same as the key before. Because of this I needed to redo the matrix with correct connections. This required a lot of time because I wasn’t familiar with keyboard PCB design.
  + Switch stabilizers not compatible with first plate design
    - The holes for the switches were too big. They stay in place but rattle a lot while pressing keys, which makes the keyboard feel cheap. The plate needs to be redesigned with more tight holes for the stabilizers.
  + Ver2 problem
    - There were few mistakes in PCB version 2. Two buttons were still tied to the same row and column, which made them register as the same button. This was fixed by cutting the column trace on the PCB and rerouting it to the correct column using jumper wire.
  + MCU package difficulties
    - MCU had a package of **asdw,** which made it difficult to solder using soldering iron. This is why it was required to learn hot air soldering. If hot air would have not been an option, it would have been impossible to assemble the MCU. The package would need to be changed to **asasd** to make the soldering viable using only soldering iron.
  + Case imperfecties
    - Only one version of the case was ever produced. Since it was the first time machining the case, imperfections were almost impossible to completely eliminate. The case came out as functional and important tolerances were met, but some machining mistakes can be seen.

All components were purchased from Digikey and PCBs from JLCPCB.

Switch design: The best option was Holy Panda switches which are advertised as the most tactile switches in the world. There was no opportunity to test these switches out, but based on the sound tests they seemed good. Unfortunately, whole set of these switches would’ve costed 70 euros, which made them inaccessible for this project.

Case machining: The price quotation from Hubs.com for the case machined would’ve been 254 euros which was completely out of budget. One possible way to stay under budget if machining is not an option would be to 3d-print the case and add dense material as weight to simulate the wanted properties.

Links:

[1] <https://drop.com/buy/drop-invyr-holy-panda-mechanical-switches?defaultSelectionIds=977750>

[2] Cherrys datasheet